1

   ABAQUS VERSION 6.6-1                                     DATE 14-Nov-2008   TIME 19:38:16
   For use by Legends Never Die under license from ABAQUS, Inc.





    AAAAAA     BBBBBBBBB      AAAAAA      QQQQQQQQ    U        U    SSSSSSSS
   A      A    B        B    A      A    Q        Q   U        U   S
  A        A   B        B   A        A   Q        Q   U        U   S
  A        A   B        B   A        A   Q        Q   U        U   S
  AAAAAAAAAA   BBBBBBBBB    AAAAAAAAAA   Q        Q   U        U    SSSSSSSS
  A        A   B        B   A        A   Q    Q   Q   U        U            S
  A        A   B        B   A        A   Q     Q  Q   U        U            S
  A        A   B        B   A        A   Q      Q Q   U        U            S
  A        A   BBBBBBBBB    A        A    QQQQQQQQ     UUUUUUUU     SSSSSSSS
 



                      This program has been developed by
 
                                  ABAQUS, Inc.
                                Rising Sun Mills
                               166 Valley Street
                         Providence, RI 02909-2499, USA
 


                   For use by Legends Never Die under license from ABAQUS, Inc. 
                   This is a proprietary program. It may only be  
                   used under the terms of the license agreement  
                   between ABAQUS, Inc. and Legends Never Die
 
                        On machine Arbeitszimmer 
                        you are authorized to run
                        ABAQUS/Standard until 31-Dec-2016

                        Your site id is: LND - 7330757468@CS 


 
                    For assistance or any other information contact

                           ABAQUS, INC.
                           1080 Main Street
                           Pawtucket, RI 02860-4847
                           U.S.A.
                           Tel: (1) 401 727 4200
                           Fax: (1) 401 727 4208
                           E-mail: info@abaqus.com
                           Web: http://www.abaqus.com
                           Technical support: support@abaqus.com 


                * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 
                *                                                         * 
                *                   *****************                     * 
                *                   *  N O T I C E  *                     * 
                *                   *****************                     * 
                *                                                         * 
                *                                                         * 
                *                 ABAQUS VERSION 6.6-1                    * 
                *                                                         * 
                *          BUILD ID: 2006_03_22-16.31.34 69548            * 
                *                                                         * 
                *                                                         * 
                *  Please make sure you are using version 6.6 manuals     * 
                *  plus the notes accompanying this release.              * 
                *                                                         * 
                *                                                         * 
                *                                                         * 
                *                                                         * 
                * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 


 



     PROCESSING PART, INSTANCE, AND ASSEMBLY INFORMATION
   *******************************************************


     END PROCESSING PART, INSTANCE, AND ASSEMBLY INFORMATION
   ***********************************************************




     OPTIONS BEING PROCESSED
   ***************************


  *Heading
  *Node
  *Element, type=C3D8
  *Nset, nset=ASSEMBLY_STAB-1__PICKEDSET4
  *Elset, elset=ASSEMBLY_STAB-1__PICKEDSET4
  *Node
  *Element, type=C3D8
  *Nset, nset=ASSEMBLY_RING-1__PICKEDSET2
  *Elset, elset=ASSEMBLY_RING-1__PICKEDSET2
  *Nset, nset=ASSEMBLY__PICKEDSET14
  *Nset, nset=ASSEMBLY__PICKEDSET65
  *Nset, nset=ASSEMBLY__PICKEDSET66
  *Elset, elset=ASSEMBLY__PICKEDSET14
  *Elset, elset=ASSEMBLY__PICKEDSET66
  *Elset, elset=ASSEMBLY__RING_S2
  *Elset, elset=ASSEMBLY__STAB_S2
  *Elset, elset=ASSEMBLY__STAB_S3
  *Elset, elset=ASSEMBLY__STAB_S4
  *Elset, elset=ASSEMBLY___PICKEDSURF72_S2
  *Elset, elset=ASSEMBLY___PICKEDSURF72_S3
  *Elset, elset=ASSEMBLY___PICKEDSURF72_S4
  *Elset, elset=ASSEMBLY___PICKEDSURF73_S2
  *tie, name="FESTER SITZ", type=SURFACETOSURFACE, adjust=YES
  *surface, type=ELEMENT, name=ASSEMBLY_STAB
  *surface, type=ELEMENT, name=ASSEMBLY_RING
  *surface, type=ELEMENT, name=ASSEMBLY__PICKEDSURF72
  *surface, type=ELEMENT, name=ASSEMBLY__PICKEDSURF73
  *tie, name="FESTER SITZ", type=SURFACETOSURFACE, adjust=YES
  *surface, type=ELEMENT, name=ASSEMBLY_STAB
  *surface, type=ELEMENT, name=ASSEMBLY_RING
  *surface, type=ELEMENT, name=ASSEMBLY__PICKEDSURF72
  *surface, type=ELEMENT, name=ASSEMBLY__PICKEDSURF73
  *surface, type=ELEMENT, name=ASSEMBLY_STAB
  *surface, type=ELEMENT, name=ASSEMBLY_RING
  *surface, type=ELEMENT, name=ASSEMBLY__PICKEDSURF72
  *surface, type=ELEMENT, name=ASSEMBLY__PICKEDSURF73
  *tie, name="FESTER SITZ", type=SURFACETOSURFACE, adjust=YES
  *tie, name="FESTER SITZ", type=SURFACETOSURFACE, adjust=YES
  *material, name=TITAN
  *elastic
  *solidsection, elset=ASSEMBLY_STAB-1__PICKEDSET4, material=TITAN
  *solidsection, elset=ASSEMBLY_RING-1__PICKEDSET2, material=TITAN
  *tie, name="FESTER SITZ", type=SURFACETOSURFACE, adjust=YES
  *boundary
  *boundary
  *tie, name="FESTER SITZ", type=SURFACETOSURFACE, adjust=YES


  SLAVE : ASSEMBLY__PICKEDSURF73                                                          
  MASTER: ASSEMBLY__PICKEDSURF72                                                          
              DISTANCE
   NODE       ADJUSTED    REMARKS/WARNINGS

         7   3.95441E-02  ADJUSTED TO ( -4.9507    , -10.000    , 0.31147    ).
         8   3.95441E-02  ADJUSTED TO ( -4.9507    , -6.0000    , 0.31147    ).
         9   3.95441E-02  ADJUSTED TO ( -4.9507    , -2.0000    , 0.31147    ).
        10   3.95441E-02  ADJUSTED TO ( -4.9507    ,  2.0000    , 0.31147    ).
        11   3.95441E-02  ADJUSTED TO ( -4.9507    ,  6.0000    , 0.31147    ).
        12   3.95441E-02  ADJUSTED TO ( -4.9507    ,  10.000    , 0.31147    ).
        13   5.91206E-02  ADJUSTED TO ( -4.9019    , -10.000    , 0.61926    ).
        14   5.91206E-02  ADJUSTED TO ( -4.9019    , -6.0000    , 0.61926    ).
        15   5.91206E-02  ADJUSTED TO ( -4.9019    , -2.0000    , 0.61926    ).
        16   5.91206E-02  ADJUSTED TO ( -4.9019    ,  2.0000    , 0.61926    ).
        17   5.91206E-02  ADJUSTED TO ( -4.9019    ,  6.0000    , 0.61926    ).
        18   5.91206E-02  ADJUSTED TO ( -4.9019    ,  10.000    , 0.61926    ).
        19   5.91203E-02  ADJUSTED TO ( -4.8534    , -10.000    , 0.92583    ).
        20   5.91203E-02  ADJUSTED TO ( -4.8534    , -6.0000    , 0.92583    ).
        21   5.91203E-02  ADJUSTED TO ( -4.8534    , -2.0000    , 0.92583    ).
        22   5.91203E-02  ADJUSTED TO ( -4.8534    ,  2.0000    , 0.92583    ).
        23   5.91203E-02  ADJUSTED TO ( -4.8534    ,  6.0000    , 0.92583    ).
        24   5.91203E-02  ADJUSTED TO ( -4.8534    ,  10.000    , 0.92583    ).
        25   3.95443E-02  ADJUSTED TO ( -4.8046    , -10.000    ,  1.2336    ).
        26   3.95443E-02  ADJUSTED TO ( -4.8046    , -6.0000    ,  1.2336    ).




 ***WARNING: FOR *TIE PAIR (ASSEMBLY__PICKEDSURF73-ASSEMBLY__PICKEDSURF72), NOT 
             ALL THE NODES THAT HAVE BEEN ADJUSTED WERE PRINTED. SPECIFY 
             *PREPRINT,MODEL=YES FOR COMPLETE PRINTOUT.

 ***WARNING: FOR *TIE PAIR (ASSEMBLY__PICKEDSURF73-ASSEMBLY__PICKEDSURF72), 
             ADJUSTED NODES WITH VERY SMALL ADJUSTMENTS WERE NOT PRINTED. 
             SPECIFY *PREPRINT,MODEL=YES FOR COMPLETE PRINTOUT.
  *tie, name="FESTER SITZ", type=SURFACETOSURFACE, adjust=YES
  *tie, name="FESTER SITZ", type=SURFACETOSURFACE, adjust=YES
  *solidsection, elset=ASSEMBLY_STAB-1__PICKEDSET4, material=TITAN
  *solidsection, elset=ASSEMBLY_RING-1__PICKEDSET2, material=TITAN
  *surface, type=ELEMENT, name=ASSEMBLY_STAB
  *surface, type=ELEMENT, name=ASSEMBLY_RING
  *surface, type=ELEMENT, name=ASSEMBLY__PICKEDSURF72
  *surface, type=ELEMENT, name=ASSEMBLY__PICKEDSURF73
  *tie, name="FESTER SITZ", type=SURFACETOSURFACE, adjust=YES
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *Step, name=Step-1, nlgeom=YES
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *Step, name=Step-2, nlgeom=YES
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *Step, name=Step-3, nlgeom=YES
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *Step, name=Step-1, nlgeom=YES
  *Step, name=Step-2, nlgeom=YES
  *Step, name=Step-3, nlgeom=YES
  *Step, name=Step-1, nlgeom=YES
  *static
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *endstep
  *Step, name=Step-2, nlgeom=YES
  *static
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *endstep
  *Step, name=Step-3, nlgeom=YES
  *static
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *endstep
  *boundary
  *boundary
  *Step, name=Step-1, nlgeom=YES
  *static
  *cload
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *endstep
  *Step, name=Step-2, nlgeom=YES
  *static
  *cload
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *endstep
  *Step, name=Step-3, nlgeom=YES
  *static
  *cload, op=NEW
  *output, field, variable=PRESELECT
  *output, history, variable=PRESELECT
  *endstep

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 1 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 2 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 3 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 4 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 5 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 6 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 301 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 302 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 303 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 304 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 305 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 306 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: 12 nodes have dof on which incorrect boundary conditions may have 
             been specified. The nodes have been identified in node set 
             WarnNodeBCIncorrectDof.

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 1 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 2 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 3 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 4 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 5 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 6 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 301 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 302 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 303 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 304 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 305 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 306 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: 12 nodes have dof on which incorrect boundary conditions may have 
             been specified. The nodes have been identified in node set 
             WarnNodeBCIncorrectDof.

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 1 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 2 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 3 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 4 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 5 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 6 INSTANCE RING-1 
             BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 301 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 302 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 303 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 304 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 305 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: DEGREE OF FREEDOM 3 HAS BEEN ELIMINATED AT NODE 306 INSTANCE 
             RING-1 BOUNDARY CONDITION TYPE ZSYMM MAY NOT BE APPLIED AT THIS 
             NODE

 ***WARNING: 12 nodes have dof on which incorrect boundary conditions may have 
             been specified. The nodes have been identified in node set 
             WarnNodeBCIncorrectDof.



                            P R O B L E M   S I Z E


          NUMBER OF ELEMENTS IS                                  1730
          NUMBER OF NODES IS                                     2592
          NUMBER OF NODES DEFINED BY THE USER                    2592
          TOTAL NUMBER OF VARIABLES IN THE MODEL                 7776
          (DEGREES OF FREEDOM PLUS ANY LAGRANGE MULTIPLIER VARIABLES)



                              END OF USER INPUT PROCESSING



     JOB TIME SUMMARY
       USER TIME (SEC)      =  0.80000    
       SYSTEM TIME (SEC)    =  0.20000    
       TOTAL CPU TIME (SEC) =   1.0000    
       WALLCLOCK TIME (SEC) =          2
1

   ABAQUS VERSION 6.6-1                                     DATE 14-Nov-2008   TIME 19:38:25
   For use by Legends Never Die under license from ABAQUS, Inc.

                                                                                               STEP    1  INCREMENT    1
                                                                                          TIME COMPLETED IN THIS STEP   0.00    


                        S T E P       1     S T A T I C   A N A L Y S I S


                                                                                          

     AUTOMATIC TIME CONTROL WITH -
          A SUGGESTED INITIAL TIME INCREMENT OF                1.000E-04
          AND A TOTAL TIME PERIOD OF                            1.00    
          THE MINIMUM TIME INCREMENT ALLOWED IS                1.000E-12
          THE MAXIMUM TIME INCREMENT ALLOWED IS                 1.00    

     LINEAR EQUATION SOLVER TYPE         DIRECT SPARSE

          LARGE DISPLACEMENT THEORY WILL BE USED



 STEP     1, INCREMENT          1, TIME INCREMENT=         0.100E-03, TOTAL TIME=         0.100E-03
 REORDERING OF EQUATIONS TO MINIMIZE WAVEFRONT HAS CHANGED THE MEMORY AND DISK ESTIMATES TO:
  
                   M E M O R Y   A N D   D I S K   E S T I M A T E
            SUMMARY FOR CURRENT NODE ORDERING  (STEP 1  TO  STEP 3)
  
          (NOTE THAT IF NODE ORDERING CHANGES THE SIZE ESTIMATES FOR THE STEPS WILL CHANGE)
  
  
           STEP   MAXIMUM DOF     FLOATING PT    MINIMUM MEMORY      MEMORY TO      REQUIRED DISKSPACE
                  WAVEFRONT       OPERATIONS       REQUIRED        MINIMIZE I/O
                                PER ITERATION     (MBYTES)           (MBYTES)          (MBYTES)
  
             1         528        4.02E+008         10.15              22.12             20.27
             2         528        4.02E+008         10.15              22.12             20.27
             3         528        4.02E+008         10.15              22.12             20.27
          ----    ---------      ------------    -------------     -------------      -------------
           MAX         528        4.02E+008         10.15              22.12             20.27
  
  
          THE TABLE ABOVE PROVIDES A STEP BY STEP SUMMARY OF SOME BASIC SIZING INFORMATION
          FOR THE PROBLEM. SOME FURTHER DESCRIPTION OF THE PARAMETERS GIVEN FOLLOWS:
  
          (1) MAXIMUM DOF WAVEFRONT - SIZE OF THE BIGGEST FRONT IN THE EQUATION SOLVER.
              PROVIDES A BASIC SIZING OF THE MOST MEMORY INTENSIVE SEGMENT OF SOLVER.
          (2) FLOATING POINT OPERATIONS PER ITERATION - MEASURE OF THE NUMBER OF FLOATING
              POINT OPERATIONS REQUIRED FOR A SINGLE SOLVER PASS. ON A GIVEN PLATFORM
              THE TIME REQUIRED FOR A SOLVER PASS WILL BE ROUGHLY A LINEAR FUNCTION
              OF THIS VALUE.
              NOTE - EXCEPT FOR THE FIRST STEP, THE VALUE IN THIS TABLE DOES NOT INCLUDE
                     ADDITIONAL FLOATING POINT OPERATIONS THAT ARE REQUIRED IN MULTIPLE LOAD
                     CASE STEPS WHEN CONSTRAINTS CHANGE FROM LOAD CASE TO LOAD CASE.  THIS
                     SITUATION CAUSES A REORDERING TO BE PERFORMED, AT WHICH TIME AN UPPER
                     BOUND ON THE NUMBER OF ADDITIONAL FLOATING POINT OPERATIONS WILL BE
                     CALCULATED AND INCLUDED UNDER THE ESTIMATE SUMMARIES FOR THE RELEVANT
                     STEPS (SEE NOTE BELOW ON REORDERING).
          (3) MINIMUM MEMORY REQUIRED - MINIMUM POSSIBLE MEMORY VALUE FOR standard_memory
              THAT ENABLES ABAQUS TO SOLVE THE PROBLEM. USE OF MEMORY WILL BE MINIMIZED BY
              WRITING AS MUCH INFORMATION AS POSSIBLE TO DISK WHICH WILL INCREASE I/O TIME.
          (4) MEMORY TO MINIMIZE I/O - VALUE OF standard_memory THAT ALLOWS ABAQUS TO KEEP
              ALL SIGNIFICANT SCRATCH FILES IN MEMORY. THIS WILL MINIMIZE I/O TIME FOR THE USER
              WITH ACCESS TO A LARGE AMOUNT OF MEMORY.
          (5) REQUIRED DISKSPACE - AMOUNT OF DISK REQUIRED FOR SCRATCH FILES. THESE WILL BE
              DELETED AT THE END OF THE ANALYSIS.
  
  
           NOTE - WHENEVER POSSIBLE THE USER SHOULD SET standard_memory TO BE LESS THAN THE
          PHYSICAL MEMORY ON THE MACHINE. UNLESS NECESSARY USERS SHOULD NOT MAKE USE
          OF VIRTUAL MEMORY EVEN IN AN ATTEMPT TO KEEP SCRATCH FILES IN MEMORY.
  
           NOTE - IF A REORDERING IS PERFORMED (THIS WILL ONLY GENERALLY BE DONE FOR FINITE-
          SLIDING CONTACT PROBLEMS), THE SIZE ESTIMATES DONE AT THIS TIME WILL NO LONGER 
          BE VALID. THE ESTIMATES WILL BE REDONE IN THE EVENT OF A REORDERING AND A NEW 
          SUMMARY WILL BE PRINTED FOR THE REMAINING STEPS.
  
  
  
           S I Z E   E S T I M A T E S   F O R   C U R R E N T   S T E P
  
          NUMBER OF EQUATIONS                        7776
          MAX DOF WAVEFRONT                          528
          FLOATING POINT OPS PER SOLVER ITERATION   4.02E+008
          MEMORY USED FOR STEP                     256.00 MBYTES
  
  
           ESTIMATED FILE SIZES
  
           FILE           MWORDS           MBYTES
  
          unit 10          0.010            0.078
          .fct             1.558           11.889
          .nck             0.052            0.394
          .opr             1.036            7.906
          -------        -------          -------
           TOTAL           2.656           20.267
  
1

   ABAQUS VERSION 6.6-1                                     DATE 14-Nov-2008   TIME 19:40:00
   For use by Legends Never Die under license from ABAQUS, Inc.

                                                                                               STEP    2  INCREMENT    1
                                                                                          TIME COMPLETED IN THIS STEP   0.00    


                        S T E P       2     S T A T I C   A N A L Y S I S


                                                                                          

     AUTOMATIC TIME CONTROL WITH -
          A SUGGESTED INITIAL TIME INCREMENT OF                1.000E-04
          AND A TOTAL TIME PERIOD OF                            1.00    
          THE MINIMUM TIME INCREMENT ALLOWED IS                1.000E-10
          THE MAXIMUM TIME INCREMENT ALLOWED IS                 1.00    

     LINEAR EQUATION SOLVER TYPE         DIRECT SPARSE

          LARGE DISPLACEMENT THEORY WILL BE USED
  
                   M E M O R Y   A N D   D I S K   E S T I M A T E
  
  
           S I Z E   E S T I M A T E S   F O R   C U R R E N T   S T E P
  
          NUMBER OF EQUATIONS                        7776
          MAX DOF WAVEFRONT                          528
          FLOATING POINT OPS PER SOLVER ITERATION   4.02E+008
          MEMORY USED FOR STEP                     256.00 MBYTES
  
  
           ESTIMATED FILE SIZES
  
           FILE           MWORDS           MBYTES
  
          unit 10          0.010            0.078
          .fct             1.558           11.889
          .nck             0.052            0.394
          .opr             1.036            7.906
          -------        -------          -------
           TOTAL           2.656           20.267
  
1

   ABAQUS VERSION 6.6-1                                     DATE 14-Nov-2008   TIME 19:41:24
   For use by Legends Never Die under license from ABAQUS, Inc.

                                                                                               STEP    3  INCREMENT    1
                                                                                          TIME COMPLETED IN THIS STEP   0.00    


                        S T E P       3     S T A T I C   A N A L Y S I S


                                                                                          

     AUTOMATIC TIME CONTROL WITH -
          A SUGGESTED INITIAL TIME INCREMENT OF                 1.00    
          AND A TOTAL TIME PERIOD OF                            1.00    
          THE MINIMUM TIME INCREMENT ALLOWED IS                1.000E-08
          THE MAXIMUM TIME INCREMENT ALLOWED IS                 1.00    

     LINEAR EQUATION SOLVER TYPE         DIRECT SPARSE

          LARGE DISPLACEMENT THEORY WILL BE USED
  
                   M E M O R Y   A N D   D I S K   E S T I M A T E
  
  
           S I Z E   E S T I M A T E S   F O R   C U R R E N T   S T E P
  
          NUMBER OF EQUATIONS                        7776
          MAX DOF WAVEFRONT                          528
          FLOATING POINT OPS PER SOLVER ITERATION   4.02E+008
          MEMORY USED FOR STEP                     256.00 MBYTES
  
  
           ESTIMATED FILE SIZES
  
           FILE           MWORDS           MBYTES
  
          unit 10          0.010            0.078
          .fct             1.558           11.889
          .nck             0.052            0.394
          .opr             1.036            7.906
          -------        -------          -------
           TOTAL           2.656           20.267
  


          THE ANALYSIS HAS BEEN COMPLETED



                              ANALYSIS COMPLETE
                              WITH    41 WARNING MESSAGES ON THE DAT FILE



     JOB TIME SUMMARY
       USER TIME (SEC)      =   68.900    
       SYSTEM TIME (SEC)    =   8.9000    
       TOTAL CPU TIME (SEC) =   77.800    
       WALLCLOCK TIME (SEC) =        188
